**C64 PSU Global Rev. 0**

**Testing**

The testing is still preliminary.

The testing was performed with a prototype configured for the 230V/115V option at 230V mains voltage. The output voltage was observed while being connected to load resistors for one hour. A C64 was powered (ASSY250469).

A test with 115V was not yet performed.

The 230V only transformer (TR2) fits the footprint on the PCB. This option has not been built, yet and not been tested.